---------------------------------------------------------------
     xeBuild v1.15.708
---------------------------------------------------------------
base path changed to C:\Users\Ty\Desktop\14444\11aa\xeBuild_GUI_2.094 (17150)\xeBuild_GUI_2.094 (17150)\files
---- { Image Build Mode } ----
<enter> key on completion suppressed
building glitch2 image
per build directory overridden from command line to 'data\'
data directory overridden from command line to '17349\'
1BL key overridden from command line, not looking for 1blkey.txt
1BL Key set to  : 0xDD88AD0C9ED669E7B56794FB68563EFA sum: 0x983 (expects: 0x983)
xex Key set to  : 0x20B185A59D28FDC340583FBB0896BF91 sum: 0x800 (expects: 0x800)
CPU key overridden from command line, not looking for cpukey.txt
CPU Key set to: 0xB84381E4B69DE49568AB6A57553202C9 (weight:0x35 valid; ecd: valid)
file name overridden from command line to 'output.bin'

------ parsing user ini at 'data\options.ini' ------

******* WARNING: could not open user ini at 'data\options.ini', skipping
default console DVD eject button is being used to start xell

------ parsing ini at '17349\_glitch2.ini' ------
ini version 17335

ini: label [falconbl] found
found (1) 'cba_5772.bin' crc: 0xe3696f7e
found (2) 'cbb_5772.bin' crc: 0xfb5ab9a4
found (3) 'cd_9452.bin' crc: 0x455fa02c
found (4) 'ce_1888.bin' crc: 0xff9b60df
found (5) 'cf_17349.bin' crc: 0x2214497c
found (6) 'cg_17349.bin' crc: 0xd68555aa
ini dictates dual CB for this model

[rawpatch] label not found in ini

ini: label [flashfs] found
found (1) 'aac.xexp' crc: 0xf8eb9fc2
found (2) 'bootanim.xex' crc: 0x5927de8b
found (3) 'createprofile.xex' crc: 0x150e2fd2
found (4) 'dash.xex' crc: 0x78a4c4b1
found (5) 'deviceselector.xex' crc: 0xd213aa7d
found (6) 'gamerprofile.xex' crc: 0x75baa3a4
found (7) 'hud.xex' crc: 0xddf5d430
found (8) 'huduiskin.xex' crc: 0x3f40ca47
found (9) 'mfgbootlauncher.xex' crc: 0x35ebb139
found (10) 'minimediaplayer.xex' crc: 0x21071346
found (11) 'nomni.xexp' crc: 0x48549239
found (12) 'nomnifwk.xexp' crc: 0x7e7b8333
found (13) 'nomnifwm.xexp' crc: 0xb3f9b73a
found (14) 'SegoeXbox-Light.xtt' crc: 0xe0ee6049
found (15) 'signin.xex' crc: 0x6eba3ee8
found (16) 'updater.xex' crc: 0xd915f51f
found (17) 'vk.xex' crc: 0x21315915
found (18) 'xam.xex' crc: 0xed837c51
found (19) 'xenonclatin.xtt' crc: 0xd5d17ff5
found (20) 'xenonclatin.xttp' crc: 0x7a507ad1
found (21) 'xenonjklatin.xtt' crc: 0xdde4a14c
found (22) 'xenonjklatin.xttp' crc: 0xe2adddfb
found (23) 'ximecore.xex' crc: 0xf040324c
found (24) 'ximedic.xex' crc: 0x1d992bfb
found (25) 'ximedic.xexp' crc: 0x7825f71a
found (26) '..\launch.xex' crc: 0x00000000
found (27) '..\lhelper.xex' crc: 0x00000000

ini: label [security] found
found (1) 'crl.bin' crc: 0x00000000
found (2) 'dae.bin' crc: 0x00000000
found (3) 'extended.bin' crc: 0x00000000
found (4) 'fcrt.bin' crc: 0x00000000
found (5) 'secdata.bin' crc: 0x00000000
------ ini parsing completed ------

output name overridden to: output.bin

1BL RSA pub key file is not available, signature checks will not be performed
PIRS RSA pub key file is not available, signature checks will not be performed
MASTER RSA pub key file is not available, signature checks will not be performed

------ Checking data\nanddump.bin ------
data\nanddump.bin file size: 0x1080000
nanddump header checks passed OK!
Loading NAND dump (0x1080000 bytes)...done!
Detecting NAND controller type from dump data...
	NAND dump is from a small block machine
	NAND dump uses small block controller
parsing dump into user and spare...
bad block at 0x2ce (raw offset 0xb91c00), block ignored
copying nanddump data from block 0x3fe to block 0x2ce for file extraction integrity
block 0x2ce was remapped to block 0x3fe at remap instance 0
done!
cleaning up stray remaps
done!
--remap summary--
0: source: 0x02ce dest: 0x03fe
-----------------
decrypting KeyVault at address 0x4000 of size 0x4000
keyvault decrypted OK, will use if no kv.bin is provided
decrypting SMC at address 0x1000 of size 0x3000
SMC decrypted OK, will use if no external smc.bin is provided
seeking smc config in dump...found at offset 0xf7c000! Using if no smc config is provided.
CF slot 0 decrypted ok LDV 0x1d Pairing: 0xfa34fc
setting LDV from image to 29
setting pairing data from image to 0xfa34fc
pairing set to: fa 34 fc
Scanning for mobile data and fsroot...Mobiles found:
    fsroot      version 01 found at offset 0x00e30000 len 0x4000 page 0x00007180
seeking security files...
crl.bin found in sector 0x388 size 0x190...verified! Will use if external file not found.
dae.bin found in sector 0x389 size 0x2c0...verified! Will use if external file not found.
extended.bin found in sector 0x38a size 0x4000...verified! Will use if external file not found.
secdata.bin found in sector 0x38b size 0x400...verified! Will use if external file not found.
done!
Writing initial header to flash image

------ loading system update container ------
17349\su20076000_00000000 found, loading...done!
	Read 0xb3d000 bytes to memory
checking integrity...
header seems valid, version 2.0.17349.0
header hash is OK, checking content hashes...
content hashes seem OK, everything looks good!
extracted SUPD\xboxupd.bin (0x7a410 bytes)
decrypting SUPD\xboxupd.bin\CF_17349.bin (0x4560 bytes)...done!
decrypting SUPD\xboxupd.bin\CG_17349.bin (0x75ea2 bytes)...done!

------ Loading bootloaders and required security files ------
reading data\smc.bin failed, using smc.bin from nand dump
reset smc load address to 0x1000 size 0x3000
reading data\kv.bin failed, using kv.bin from nand dump
reading .\common\cba_5772.bin (0x1ac0 bytes)
loaded cba_5772.bin, could not check signature rsa key not present!
reading .\common\cbb_5772.bin (0x9350 bytes)
reading .\common\cd_9452.bin (0x4f20 bytes)
reading .\common\ce_1888.bin (0x5606a b pad 0x56070 b)
xell not found in perbuild directory, checking firmware /bin folder
xell not found in firmware /bin folder, checking base path
reading xell-gggggg.bin (0x40000 bytes)
extracted SUPD\xboxupd.bin\CF_17349.bin (0x4560 bytes)
extracted SUPD\xboxupd.bin\CG_17349.bin (0x75ea2 bytes)
reading 17349\bin\patches_g2falcon.bin (0x91c bytes)
reading data\smc_config.bin failed, using smc_config.bin from nand dump
-------------------
checking smc_config
-------------------
extracting config
------------------
SMC config info:
------------------
Target temps: Cpu:  80øC Gpu:  75øC Edram:  78øC
Max temps   : Cpu: 100øC Gpu: 100øC Edram: 102øC
Cpu Fan     : (auto)
Gpu Fan     : (auto)
MAC Address : 00:22:48:62:7a:2e
AVRegion    : 0x00000100 (NTSC-M)
GameRegion  : 0x00ff (NTSC/US)
DVDRegion   : 1
resetKey    : LLDX
---------------------
Checking for smc config data patches
smc config was not patched
---------------------
could not check signature of cba_5772.bin, 1BL RSA key not present!
done!
patch slot offset reset to: 0xb0000

------ Patching BLs and modifying patches ------
Patching BLs...Done!

------ Patching boot reasons and options into flash header ------
	Patching header for xell power reason

------ Encrypting and finalizing bootloaders ------
encoding smc.bin size 0x3000
SMC checksum: 45ebe68a
unknown SMC found, type: Falcon v3.1(1.06)
glitch hack found in SMC binary!
encoding kv.bin size 0x4000
decrypted keyvault has been set for reference
Master RSA pub not available, not checking hash
encoding cba_5772.bin size 0x1ac0
encoding cbb_5772.bin size 0x9350
CB 5772 seq 0x010800d8 type: 0x01 cseq: 0x08 allow: 0x00d8
	expected fuses:
	fuseset 00: C0FFFFFFFFFFFFFF
	fuseset 01: 0F0F0F0F0F0F0FF0 (retail)
	fuseset 02: 0000000F00000000 (sequence)
	fuseset 02: 000F000000000000 (allow cseq 4)
	fuseset 02: 0000F00000000000 (allow cseq 5)
	fuseset 02: 000000F000000000 (allow cseq 7)
	fuseset 02: 0000000F00000000 (allow cseq 8)
	**dual CB flag detected!**
encoding cd_9452.bin size 0x5290
encoding ce_1888.bin size 0x56070
encoding xell-gggggg.bin size 0x40000
encoding cf_17349.bin size 0x4560
encoding cg_17349.bin size 0x75eb0
encoding patches_g2falcon.bin size 0x550
done!

------ Adding bootloaders to flash image ------
adding smc.bin at raw offset 0x00001000 len 0x3000 (end 0x4000)
adding kv.bin at raw offset 0x00004000 len 0x4000 (end 0x8000)
adding cba_5772.bin at raw offset 0x00008000 len 0x1ac0 (end 0x9ac0)
adding cbb_5772.bin at raw offset 0x00009ac0 len 0x9350 (end 0x12e10)
adding cd_9452.bin at raw offset 0x00012e10 len 0x5290 (end 0x180a0)
adding ce_1888.bin at raw offset 0x000180a0 len 0x56070 (end 0x6e110)
adding xell-gggggg.bin at raw offset 0x00070000 len 0x40000 (end 0xb0000)
adding cf_17349.bin at raw offset 0x000b0000 len 0x4560 (end 0xb4560)
adding cg_17349.bin at raw offset 0x000b4560 len 0x75eb0 (end 0xc0000, rest in fs)
adding patches_g2falcon.bin at raw offset 0x000c0010 len 0x550 (end 0xc0560)
Fixing up FS table...done!
Writing zeropair CG patch slot overflow data to sysupdate.xexp1
	at raw offset 0xd0000 len 0x0006a410 (end: 0x0013a410)...done!

------ adding 27 firmware files ------
extracted SUPD\aac.xexp (0x14000 bytes) (crc32: 0xf8eb9fc2 ini: 0xf8eb9fc2)
	adding as aac.xexp1 at raw offset 0x13a410 len 0x00014000 (end 0x0014e410)
extracted SUPD\bootanim.xex (0x61000 bytes) (crc32: 0x5927de8b ini: 0x5927de8b)
	adding as bootanim.xex at raw offset 0x150000 len 0x00061000 (end 0x001b1000)
extracted SUPD\createprofile.xex (0xc000 bytes) (crc32: 0x150e2fd2 ini: 0x150e2fd2)
	adding as createprofile.xex at raw offset 0x1b1000 len 0x0000c000 (end 0x001bd000)
extracted SUPD\dash.xex (0x5a0000 bytes) (crc32: 0x78a4c4b1 ini: 0x78a4c4b1)
	adding as dash.xex at raw offset 0x1c0000 len 0x005a0000 (end 0x00760000)
extracted SUPD\deviceselector.xex (0xa000 bytes) (crc32: 0xd213aa7d ini: 0xd213aa7d)
	adding as deviceselector.xex at raw offset 0x760000 len 0x0000a000 (end 0x0076a000)
extracted SUPD\gamerprofile.xex (0x1b000 bytes) (crc32: 0x75baa3a4 ini: 0x75baa3a4)
	adding as gamerprofile.xex at raw offset 0x76a000 len 0x0001b000 (end 0x00785000)
extracted SUPD\hud.xex (0x1d000 bytes) (crc32: 0xddf5d430 ini: 0xddf5d430)
	adding as hud.xex at raw offset 0x787000 len 0x0001d000 (end 0x007a4000)
extracted SUPD\huduiskin.xex (0x14000 bytes) (crc32: 0x3f40ca47 ini: 0x3f40ca47)
	adding as huduiskin.xex at raw offset 0x7a5000 len 0x00014000 (end 0x007b9000)
extracted SUPD\mfgbootlauncher.xex (0x8000 bytes) (crc32: 0x35ebb139 ini: 0x35ebb139)
	adding as mfgbootlauncher.xex at raw offset 0x7bc000 len 0x00008000 (end 0x007c4000)
extracted SUPD\minimediaplayer.xex (0xc000 bytes) (crc32: 0x21071346 ini: 0x21071346)
	adding as minimediaplayer.xex at raw offset 0x7c4000 len 0x0000c000 (end 0x007d0000)
extracted SUPD\nomni.xexp (0xc800 bytes) (crc32: 0x48549239 ini: 0x48549239)
	adding as nomni.xexp1 at raw offset 0x7d0000 len 0x0000c800 (end 0x007dc800)
extracted SUPD\nomnifwk.xexp (0x2000 bytes) (crc32: 0x7e7b8333 ini: 0x7e7b8333)
	adding as nomnifwk.xexp1 at raw offset 0x7dc800 len 0x00002000 (end 0x007de800)
extracted SUPD\nomnifwm.xexp (0x5000 bytes) (crc32: 0xb3f9b73a ini: 0xb3f9b73a)
	adding as nomnifwm.xexp1 at raw offset 0x7e2000 len 0x00005000 (end 0x007e7000)
extracted SUPD\SegoeXbox-Light.xtt (0x6000 bytes) (crc32: 0xe0ee6049 ini: 0xe0ee6049)
	adding as SegoeXbox-Light.xtt at raw offset 0x7e9000 len 0x00006000 (end 0x007ef000)
extracted SUPD\signin.xex (0x1a000 bytes) (crc32: 0x6eba3ee8 ini: 0x6eba3ee8)
	adding as signin.xex at raw offset 0x7f2000 len 0x0001a000 (end 0x0080c000)
extracted SUPD\updater.xex (0x7000 bytes) (crc32: 0xd915f51f ini: 0xd915f51f)
	adding as updater.xex at raw offset 0x80e000 len 0x00007000 (end 0x00815000)
extracted SUPD\vk.xex (0xb000 bytes) (crc32: 0x21315915 ini: 0x21315915)
	adding as vk.xex at raw offset 0x817000 len 0x0000b000 (end 0x00822000)
extracted SUPD\xam.xex (0x252000 bytes) (crc32: 0xed837c51 ini: 0xed837c51)
	adding as xam.xex at raw offset 0x823000 len 0x00252000 (end 0x00a75000)
extracted nanddump\xenonclatin.xtt (0x11b000 bytes) (crc32: 0xd5d17ff5 ini: 0xd5d17ff5)
	adding as xenonclatin.xtt at raw offset 0xa76000 len 0x0011b000 (end 0x00b91000)
extracted SUPD\xenonclatin.xttp (0x18000 bytes) (crc32: 0x7a507ad1 ini: 0x7a507ad1)
	adding as xenonclatin.xttp1 at raw offset 0xb93000 len 0x00018000 (end 0x00bab000)
extracted nanddump\xenonjklatin.xtt (0x1a8000 bytes) (crc32: 0xdde4a14c ini: 0xdde4a14c)
	adding as xenonjklatin.xtt at raw offset 0xbac000 len 0x001a8000 (end 0x00d54000)
extracted SUPD\xenonjklatin.xttp (0x7000 bytes) (crc32: 0xe2adddfb ini: 0xe2adddfb)
	adding as xenonjklatin.xttp1 at raw offset 0xd54000 len 0x00007000 (end 0x00d5b000)
extracted SUPD\ximecore.xex (0x17000 bytes) (crc32: 0xf040324c ini: 0xf040324c)
	adding as ximecore.xex at raw offset 0xd5b000 len 0x00017000 (end 0x00d72000)
extracted nanddump\ximedic.xex (0x90000 bytes) (crc32: 0x1d992bfb ini: 0x1d992bfb)
	adding as ximedic.xex at raw offset 0xd73000 len 0x00090000 (end 0x00e03000)
extracted SUPD\ximedic.xexp (0x2800 bytes) (crc32: 0x7825f71a ini: 0x7825f71a)
	adding as ximedic.xexp1 at raw offset 0xe04000 len 0x00002800 (end 0x00e06800)
reading 17349\..\launch.xex (0xd000 bytes)
	adding as launch.xex at raw offset 0xe06800 len 0x0000d000 (end 0x00e13800)
reading 17349\..\lhelper.xex (0x6000 bytes)
	adding as lhelper.xex at raw offset 0xe15000 len 0x00006000 (end 0x00e1b000)

------ adding 5 security files ------
<- Processing crl.bin ->
reading data\crl.bin (0xa00 bytes)
crl appears crypted, attempting to decrypt with CPU key...failed! Trying alternate key...success!
	adding as crl.bin at raw offset 0xe20000 len 0x00000a00 (end 0x00e20a00)

<- Processing dae.bin ->
reading data\dae.bin (0xad30 bytes)
dae appears encrypted, attempting to decrypt with CPU key...failed! Attempting to decrypt with alternate key...
success!
	adding as dae.bin at raw offset 0xe24000 len 0x0000ad30 (end 0x00e2ed30)

<- Processing extended.bin ->
reading data\extended.bin (0x4000 bytes)
	adding as extended.bin at raw offset 0xe30000 len 0x00004000 (end 0x00e34000)

<- Processing fcrt.bin ->
	fcrt.bin not found and not required by keyvault, skipped

<- Processing secdata.bin ->
reading data\secdata.bin (0x400 bytes)
	adding as secdata.bin at raw offset 0xe34000 len 0x00000400 (end 0x00e34400)

------ checking for Mobile*.dat ------

------ adding smc_config.bin ------
adding smc config to offset 0x00f7c000, len 0x400

------ cleaning up image ------
Fixing up empty FS block entries...done!
Writing FS table to image offset 0xe38000 len 0x4000 (end 0xe3c000)...done!

------ finalizing image ------
calculating ECD bytes and assembling raw image...done!
remapping 1 blocks
    copying 0x4200 bytes of LBA 0x2ce to block 0x3fe...zero fill origin...done!
done remapping!

------ writing image to disk ------
writing file 'output.bin' to disk...done!
---------------------------------------------------------------
output.bin image built, info:
---------------------------------------------------------------
Kernel    : 2.0.17349.0
Console   : Falcon
NAND size : 16MiB
Build     : Glitch (v2)
Xell      : power on console with console eject button
Serial    : 277552784505
ConsoleId : 030095754700
MoboSerial: 7578551115018455
Mfg Date  : 11/06/2008
CPU Key   : B84381E4B69DE49568AB6A57553202C9
1BL Key   : DD88AD0C9ED669E7B56794FB68563EFA
DVD Key   : 0DD6460615070BF5AED4256992FEFFC7
CF LDV    : 29
KV type   : type2 (hashed - unchecked, master key not available)
---------------------------------------------------------------
    xeBuild Finished. Have a nice day.
---------------------------------------------------------------
