========================================================
 xeBuild GUI v 2.094 Debuglog
 4/30/2015 12:00:00 AM 4/30/2015 4:48:00 AM
========================================================
 *** Settings variables ***
Source: D:\XBOX\Nand_Dumps\haydenFalcon\updflash_edited.bin
Output: D:\XBOX\Nand_Dumps\haydenFalcon\updflash.bin
Image Type: glitch2
Mobo: falcon
CPUKey: B84381E4B69DE49568AB6A57553202C9
1BLKey: DD88AD0C9ED669E7B56794FB68563EFA
Kernel version: 17349
Xell Version: xellreloaded
SMC Hack: currentsmc
Include Dashlaunch: True
Custom Dashlaunch settings: True
Automatic Selection: True
Custom xeBuild: True
Custom filelist/patch: False
Custom filelist/patch (Name): 
CFLDV: 
Auto Save Log: True
Auto Save Log (Dir + Name): D:\XBOX\Nand_Dumps\haydenFalcon\xeBuild_GUI.log
Simple Mode:False
Verbose xeBuild Output:True
 *** MD5 hashes ***
          xeBuild.exe: F1B2BFE4F0268F543EBEA5ABC3D20DEA
Original with release: 678C93B8642D142F78A21D8FA09C4343
           launch.xex: 866AC5FF6C766EBB76CDEC3F3561C7FB
Original with release: 9356939823865BE749333C02E1AB480D
          lhelper.xex: 494D48CFCF77570D196C11BD60210779
Original with release: F0BC94D451BA7496B9DBC7BB42882569
          build.py:    57E1D0CC5A059AF069CF7A172DEFCBD8
Original with release: 1E3BE54136B3A9DE25D2B75CC6BC8C9E

 *** Actual log ***
==================================
 Swizzy's xeBuild GUI version 2.094
 Log Started: Thursday 4/30/2015 4:47:54 AM
==================================

 *** Some console information ***
CB Version: 5772
Serial number: 277552784505
Console region: NTSC/USA (0x00FF)
DVDKey: 0DD6460615070BF5AED4256992FEFFC7
Console ID: 0B3627A2E0
MFR-Date: 06-11-08
OSIG String: PLDS    DG-16D2S        7485
FCRT.bin Required: False

Adding custom xeBuild Settings... Done!
Using xell-reloaded for Glitch hack
Including dashlaunch... Done!
Including custom dashlaunch settings (launch.ini)... Done!
Copying nand to data directory, this may take a while... Done!
Checking if SMC is Glitch or Retail...
Dumping current SMC... Done!
Checking SMC...
SMC is Glitch patched! it will be used the way it is...
Enabling Verbose mode output for xeBuild...

Parameters sent to xeBuild:

-noenter -t glitch2 -c falcon -d data -f 17349 -b DD88AD0C9ED669E7B56794FB68563EFA -p B84381E4B69DE49568AB6A57553202C9  -o gpufan=0 -o cpufan=0 -v  output.bin

Building nand using xeBuild (this may take a while):

---------------------------------------------------------------
     xeBuild v1.13.689
---------------------------------------------------------------
base path changed to C:\Users\Ty\Desktop\14444\11aa\xeBuild_GUI_2.094 (17150)\xeBuild_GUI_2.094 (17150)\files
---- { Image Build Mode } ----
building glitch2 image

verbose set to level 1
file name overridden from command line to 'output.bin'

------ parsing user ini at 'data\options.ini' ------

******* WARNING: could not open user ini at 'data\options.ini', skipping
default console DVD eject button is being used to start xell

------ parsing ini at '17349\_glitch2.ini' ------
ini version 17349

ini: label [falconbl] found
found (1) 'cba_5772.bin' crc: 0xe3696f7e
found (2) 'cbb_5772.bin' crc: 0xfb5ab9a4
found (3) 'cd_9452.bin' crc: 0x455fa02c
found (4) 'ce_1888.bin' crc: 0xff9b60df
found (5) 'cf_17349.bin' crc: 0x2214497c
found (6) 'cg_17349.bin' crc: 0xd68555aa
ini dictates dual CB for this model

ini: label [flashfs] found
found (1) 'aac.xexp' crc: 0xf8eb9fc2
found (2) 'bootanim.xex' crc: 0x5927de8b
found (3) 'createprofile.xex' crc: 0x150e2fd2
found (4) 'dash.xex' crc: 0x78a4c4b1
found (5) 'deviceselector.xex' crc: 0xd213aa7d
found (6) 'gamerprofile.xex' crc: 0x75baa3a4
found (7) 'hud.xex' crc: 0xddf5d430
found (8) 'huduiskin.xex' crc: 0x3f40ca47
found (9) 'mfgbootlauncher.xex' crc: 0x35ebb139
found (10) 'minimediaplayer.xex' crc: 0x21071346
found (11) 'nomni.xexp' crc: 0x48549239
found (12) 'nomnifwk.xexp' crc: 0x7e7b8333
found (13) 'nomnifwm.xexp' crc: 0xb3f9b73a
found (14) 'SegoeXbox-Light.xtt' crc: 0xe0ee6049
found (15) 'signin.xex' crc: 0x6eba3ee8
found (16) 'updater.xex' crc: 0xd915f51f
found (17) 'vk.xex' crc: 0x21315915
found (18) 'xam.xex' crc: 0xed837c51
found (19) 'xenonclatin.xtt' crc: 0xd5d17ff5
found (20) 'xenonclatin.xttp' crc: 0x7a507ad1
found (21) 'xenonjklatin.xtt' crc: 0xdde4a14c
found (22) 'xenonjklatin.xttp' crc: 0xe2adddfb
found (23) 'ximecore.xex' crc: 0xf040324c
found (24) 'ximedic.xex' crc: 0x1d992bfb
found (25) 'ximedic.xexp' crc: 0x7825f71a
found (26) '..\launch.xex' crc: 0x00000000
found (27) '..\lhelper.xex' crc: 0x00000000

ini: label [security] found
found (1) 'crl.bin' crc: 0x00000000
found (2) 'dae.bin' crc: 0x00000000
found (3) 'extended.bin' crc: 0x00000000
found (4) 'fcrt.bin' crc: 0x00000000
found (5) 'secdata.bin' crc: 0x00000000
------ ini parsing completed ------

output name overridden to: output.bin

1BL RSA pub key file is not available, signature checks will not be performed
PIRS RSA pub key file is not available, signature checks will not be performed
MASTER RSA pub key file is not available, signature checks will not be performed

------ Checking data\nanddump.bin ------
data\nanddump.bin file size: 0x1080000
nanddump header checks passed OK!
Loading NAND dump (0x1080000 bytes)...done!
Detecting NAND controller type from dump data...
	NAND dump is from a small block machine
	NAND dump uses small block controller
parsing dump into user and spare...
bad block at 0x2ce (raw offset 0xb91c00), block ignored
bad block at 0x3ff (raw offset 0x107be00), block ignored
done!
cleaning up stray remaps
block 0x2ce had no remap, assigning remap block 0x3fe
block 0x3ff had no need of remap, it's in the wear area
done!
--remap summary--
0: source: 0x02ce dest: 0x03fe
1: source: 0x03ff dest: (NONE/BAD)
-----------------
decrypting KeyVault at address 0x4000 of size 0x4000
keyvault decrypted OK, will use if no kv.bin is provided
decrypting SMC at address 0x1000 of size 0x3000
SMC decrypted OK, will use if no external smc.bin is provided
seeking smc config in dump...found at offset 0xf7c000! Using if no smc config is provided.
CF slot 0 decrypted ok LDV 0x1d Pairing: 0xfa34fc
setting LDV from image to 29
setting pairing data from image to 0xfa34fc
pairing set to: fa 34 fc
MobileB.dat found at block 0x387, page 0x0 (page 0x70e0), size 2048 (0x800) bytes
MobileC.dat found at block 0x388, page 0x0 (page 0x7100), size 512 (0x200) bytes
MobileD.dat found at block 0x389, page 0x0 (page 0x7120), size 2048 (0x800) bytes
MobileE.dat found at block 0x38a, page 0x0 (page 0x7140), size 2048 (0x800) bytes
Statistics.settings found at page 0x7bc0, size 4096 (0x1000) bytes
Manufacturing.data found at page 0x7bc0, size 4096 (0x1000) bytes
seeking FSRoot...fsroot found at block 0x38b, page 0x0 (page 0x7160) raw offset 0x7160
seeking security files...
crl.bin found in sector 0x381 size 0xa00...verified! Will use if external file not found.
dae.bin found in sector 0x382 size 0xad30...verified! Will use if external file not found.
extended.bin found in sector 0x385 size 0x4000...verified! Will use if external file not found.
secdata.bin found in sector 0x386 size 0x400...verified! Will use if external file not found.
done!
Writing initial header to flash image

------ loading system update container ------
17349\su20076000_00000000 found, loading...done!
	Read 0xb3d000 bytes to memory
checking integrity...
header seems valid, version 2.0.17349.0
header hash is OK, checking content hashes...
content hashes seem OK, everything looks good!
extracted SUPD\xboxupd.bin (0x7a410 bytes)
decrypting SUPD\xboxupd.bin\CF_17349.bin (0x4560 bytes)...done!
decrypting SUPD\xboxupd.bin\CG_17349.bin (0x75ea2 bytes)...done!

------ Loading bootloaders and required security files ------
reading data\smc.bin failed, using smc.bin from nand dump
reset smc load address to 0x1000 size 0x3000
reading data\kv.bin failed, using kv.bin from nand dump
reading .\common\cba_5772.bin (0x1ac0 bytes)
loaded cba_5772.bin, could not check signature rsa key not present!
reading .\common\cbb_5772.bin (0x9350 bytes)
reading .\common\cd_9452.bin (0x4f20 bytes)
reading .\common\ce_1888.bin (0x5606a b pad 0x56070 b)
xell not found in perbuild directory, checking firmware /bin folder
xell not found in firmware /bin folder, checking base path
reading xell-gggggg.bin (0x40000 bytes)
extracted SUPD\xboxupd.bin\CF_17349.bin (0x4560 bytes)
extracted SUPD\xboxupd.bin\CG_17349.bin (0x75ea2 bytes)


**** could not read patches_g2falcon.bin (-1) ****

******* ERROR: critical bootloader files are missing, cannot proceed!



***** FATAL BUILD ERROR: -1 unable to complete NAND image

---------------------------------------------------------------
    xeBuild Finished. Have a nice day.
---------------------------------------------------------------
xeBuild ERROR: image build error
ERROR: There was one or more fatal errors: 1 errors during the build process
Cleaning data and temporary directories... Done!


       ****** The app has now finished! ******



 *** xeBuild's verbose log *** 
 it was last updated: 4/30/2015 4:47:56 AM

---------------------------------------------------------------
     xeBuild v1.13.689
---------------------------------------------------------------
base path changed to C:\Users\Ty\Desktop\14444\11aa\xeBuild_GUI_2.094 (17150)\xeBuild_GUI_2.094 (17150)\files
---- { Image Build Mode } ----
<enter> key on completion suppressed
building glitch2 image
per build directory overridden from command line to 'data\'
data directory overridden from command line to '17349\'
1BL key overridden from command line, not looking for 1blkey.txt
1BL Key set to  : 0xDD88AD0C9ED669E7B56794FB68563EFA sum: 0x983 (expects: 0x983)
xex Key set to  : 0x20B185A59D28FDC340583FBB0896BF91 sum: 0x800 (expects: 0x800)
CPU key overridden from command line, not looking for cpukey.txt
CPU Key set to: 0xB84381E4B69DE49568AB6A57553202C9 (weight:0x35 valid; ecd: valid)
Using GPUFAN option, value 0
Using CPUFAN option, value 0
file name overridden from command line to 'output.bin'

------ parsing user ini at 'data\options.ini' ------

******* WARNING: could not open user ini at 'data\options.ini', skipping
default console DVD eject button is being used to start xell

------ parsing ini at '17349\_glitch2.ini' ------
ini version 17349

ini: label [falconbl] found
found (1) 'cba_5772.bin' crc: 0xe3696f7e
found (2) 'cbb_5772.bin' crc: 0xfb5ab9a4
found (3) 'cd_9452.bin' crc: 0x455fa02c
found (4) 'ce_1888.bin' crc: 0xff9b60df
found (5) 'cf_17349.bin' crc: 0x2214497c
found (6) 'cg_17349.bin' crc: 0xd68555aa
ini dictates dual CB for this model

ini: label [flashfs] found
found (1) 'aac.xexp' crc: 0xf8eb9fc2
found (2) 'bootanim.xex' crc: 0x5927de8b
found (3) 'createprofile.xex' crc: 0x150e2fd2
found (4) 'dash.xex' crc: 0x78a4c4b1
found (5) 'deviceselector.xex' crc: 0xd213aa7d
found (6) 'gamerprofile.xex' crc: 0x75baa3a4
found (7) 'hud.xex' crc: 0xddf5d430
found (8) 'huduiskin.xex' crc: 0x3f40ca47
found (9) 'mfgbootlauncher.xex' crc: 0x35ebb139
found (10) 'minimediaplayer.xex' crc: 0x21071346
found (11) 'nomni.xexp' crc: 0x48549239
found (12) 'nomnifwk.xexp' crc: 0x7e7b8333
found (13) 'nomnifwm.xexp' crc: 0xb3f9b73a
found (14) 'SegoeXbox-Light.xtt' crc: 0xe0ee6049
found (15) 'signin.xex' crc: 0x6eba3ee8
found (16) 'updater.xex' crc: 0xd915f51f
found (17) 'vk.xex' crc: 0x21315915
found (18) 'xam.xex' crc: 0xed837c51
found (19) 'xenonclatin.xtt' crc: 0xd5d17ff5
found (20) 'xenonclatin.xttp' crc: 0x7a507ad1
found (21) 'xenonjklatin.xtt' crc: 0xdde4a14c
found (22) 'xenonjklatin.xttp' crc: 0xe2adddfb
found (23) 'ximecore.xex' crc: 0xf040324c
found (24) 'ximedic.xex' crc: 0x1d992bfb
found (25) 'ximedic.xexp' crc: 0x7825f71a
found (26) '..\launch.xex' crc: 0x00000000
found (27) '..\lhelper.xex' crc: 0x00000000

ini: label [security] found
found (1) 'crl.bin' crc: 0x00000000
found (2) 'dae.bin' crc: 0x00000000
found (3) 'extended.bin' crc: 0x00000000
found (4) 'fcrt.bin' crc: 0x00000000
found (5) 'secdata.bin' crc: 0x00000000
------ ini parsing completed ------

output name overridden to: output.bin

1BL RSA pub key file is not available, signature checks will not be performed
PIRS RSA pub key file is not available, signature checks will not be performed
MASTER RSA pub key file is not available, signature checks will not be performed

------ Checking data\nanddump.bin ------
data\nanddump.bin file size: 0x1080000
nanddump header checks passed OK!
Loading NAND dump (0x1080000 bytes)...done!
Detecting NAND controller type from dump data...
	NAND dump is from a small block machine
	NAND dump uses small block controller
parsing dump into user and spare...
bad block at 0x2ce (raw offset 0xb91c00), block ignored
bad block at 0x3ff (raw offset 0x107be00), block ignored
done!
cleaning up stray remaps
block 0x2ce had no remap, assigning remap block 0x3fe
block 0x3ff had no need of remap, it's in the wear area
done!
--remap summary--
0: source: 0x02ce dest: 0x03fe
1: source: 0x03ff dest: (NONE/BAD)
-----------------
decrypting KeyVault at address 0x4000 of size 0x4000
keyvault decrypted OK, will use if no kv.bin is provided
decrypting SMC at address 0x1000 of size 0x3000
SMC decrypted OK, will use if no external smc.bin is provided
seeking smc config in dump...found at offset 0xf7c000! Using if no smc config is provided.
CF slot 0 decrypted ok LDV 0x1d Pairing: 0xfa34fc
setting LDV from image to 29
setting pairing data from image to 0xfa34fc
pairing set to: fa 34 fc
MobileB.dat found at block 0x387, page 0x0 (page 0x70e0), size 2048 (0x800) bytes
MobileC.dat found at block 0x388, page 0x0 (page 0x7100), size 512 (0x200) bytes
MobileD.dat found at block 0x389, page 0x0 (page 0x7120), size 2048 (0x800) bytes
MobileE.dat found at block 0x38a, page 0x0 (page 0x7140), size 2048 (0x800) bytes
Statistics.settings found at page 0x7bc0, size 4096 (0x1000) bytes
Manufacturing.data found at page 0x7bc0, size 4096 (0x1000) bytes
seeking FSRoot...fsroot found at block 0x38b, page 0x0 (page 0x7160) raw offset 0x7160
seeking security files...
crl.bin found in sector 0x381 size 0xa00...verified! Will use if external file not found.
dae.bin found in sector 0x382 size 0xad30...verified! Will use if external file not found.
extended.bin found in sector 0x385 size 0x4000...verified! Will use if external file not found.
secdata.bin found in sector 0x386 size 0x400...verified! Will use if external file not found.
done!
Writing initial header to flash image

------ loading system update container ------
17349\su20076000_00000000 found, loading...done!
	Read 0xb3d000 bytes to memory
checking integrity...
header seems valid, version 2.0.17349.0
header hash is OK, checking content hashes...
content hashes seem OK, everything looks good!
extracted SUPD\xboxupd.bin (0x7a410 bytes)
decrypting SUPD\xboxupd.bin\CF_17349.bin (0x4560 bytes)...done!
decrypting SUPD\xboxupd.bin\CG_17349.bin (0x75ea2 bytes)...done!

------ Loading bootloaders and required security files ------
reading data\smc.bin failed, using smc.bin from nand dump
reset smc load address to 0x1000 size 0x3000
reading data\kv.bin failed, using kv.bin from nand dump
reading .\common\cba_5772.bin (0x1ac0 bytes)
loaded cba_5772.bin, could not check signature rsa key not present!
reading .\common\cbb_5772.bin (0x9350 bytes)
reading .\common\cd_9452.bin (0x4f20 bytes)
reading .\common\ce_1888.bin (0x5606a b pad 0x56070 b)
xell not found in perbuild directory, checking firmware /bin folder
xell not found in firmware /bin folder, checking base path
reading xell-gggggg.bin (0x40000 bytes)
extracted SUPD\xboxupd.bin\CF_17349.bin (0x4560 bytes)
extracted SUPD\xboxupd.bin\CG_17349.bin (0x75ea2 bytes)


**** could not read patches_g2falcon.bin (-1) ****

******* ERROR: critical bootloader files are missing, cannot proceed!



***** FATAL BUILD ERROR: -1 unable to complete NAND image

---------------------------------------------------------------
    xeBuild Finished. Have a nice day.
---------------------------------------------------------------
