---------------------------------------------------------------
     xeBuild v1.17.785
---------------------------------------------------------------
base path changed to C:\Users\Ruben\Desktop\XeBuild\files
---- { Image Build Mode } ----
<enter> key on completion suppressed
building glitch image
per build directory overridden from command line to 'data/'
data directory overridden from command line to '17502/'
1BL key overridden from command line, not looking for 1blkey.txt
1BL Key set to  : 0xDD88AD0C9ED669E7B56794FB68563EFA sum: 0x983 (expects: 0x983)
xex Key set to  : 0x20B185A59D28FDC340583FBB0896BF91 sum: 0x800 (expects: 0x800)
CPU key overridden from command line, not looking for cpukey.txt
CPU Key set to: 0x21E0A69EB5B37CD533D13B1158C285FA (weight:0x35 valid; ecd: valid)
file name overridden from command line to 'output.bin'

------ parsing user ini at 'data/options.ini' ------

******* WARNING: could not open user ini at 'data/options.ini', skipping
default console DVD eject button is being used to start xell

------ parsing ini at '17502/_glitch.ini' ------
ini version 17502

ini: label [trinitybl] found
found (1) 'cba_9188.bin' crc: 0x5a76752d
found (2) 'cbb_9188.bin' crc: 0xfebb1074
found (3) 'cd_9452.bin' crc: 0x455fa02c
found (4) 'ce_1888.bin' crc: 0xff9b60df
found (5) 'cf_17502.bin' crc: 0xf0945b64
found (6) 'cg_17502.bin' crc: 0x2ae7e415
ini dictates dual CB for this model

[rawpatch] label not found in ini

ini: label [flashfs] found
found (1) 'aac.xexp' crc: 0xfa1723e0
found (2) 'bootanim.xex' crc: 0xe36c0e40
found (3) 'createprofile.xex' crc: 0xf24539bc
found (4) 'dash.xex' crc: 0x016f607b
found (5) 'deviceselector.xex' crc: 0x183f4179
found (6) 'gamerprofile.xex' crc: 0x3feefc28
found (7) 'hud.xex' crc: 0x753a9018
found (8) 'huduiskin.xex' crc: 0xd52ba633
found (9) 'mfgbootlauncher.xex' crc: 0xc8d1c074
found (10) 'minimediaplayer.xex' crc: 0x4a53b32a
found (11) 'nomni.xexp' crc: 0x97e79156
found (12) 'nomnifwk.xexp' crc: 0xfd20ebe8
found (13) 'nomnifwm.xexp' crc: 0x01314c49
found (14) 'SegoeXbox-Light.xtt' crc: 0xe0ee6049
found (15) 'signin.xex' crc: 0x980c003b
found (16) 'updater.xex' crc: 0x5f4cfb19
found (17) 'vk.xex' crc: 0xc2ee56b2
found (18) 'xam.xex' crc: 0x68901e82
found (19) 'xenonclatin.xtt' crc: 0xd5d17ff5
found (20) 'xenonclatin.xttp' crc: 0x7a507ad1
found (21) 'xenonjklatin.xtt' crc: 0xdde4a14c
found (22) 'xenonjklatin.xttp' crc: 0xe2adddfb
found (23) 'ximecore.xex' crc: 0xe232d096
found (24) 'ximedic.xex' crc: 0x1d992bfb
found (25) 'ximedic.xexp' crc: 0xfd78a3a8
found (26) '..\launch.xex' crc: 0x00000000
found (27) '..\lhelper.xex' crc: 0x00000000
found (28) '..\launch.ini' crc: 0x00000000

ini: label [security] found
found (1) 'crl.bin' crc: 0x00000000
found (2) 'dae.bin' crc: 0x00000000
found (3) 'extended.bin' crc: 0x00000000
found (4) 'fcrt.bin' crc: 0x00000000
found (5) 'secdata.bin' crc: 0x00000000
------ ini parsing completed ------

output name overridden to: output.bin

1BL RSA pub key (1BL_pub.bin) not available, signature checks will not be performed
PIRS RSA pub key (PIRS_pub.bin) not available, signature checks will not be performed
MASTER RSA pub key (MAST_pub.bin) not available, signature checks will not be performed

------ Checking data/nanddump.bin ------
data/nanddump.bin file size: 0x1080000
nanddump header checks passed OK!
Loading NAND dump (0x1080000 bytes)...done!
Detecting NAND controller type from dump data...
	NAND dump is from a small block machine
	NAND dump uses big block controller
parsing dump into user and spare...
done!
decrypting KeyVault at address 0x4000 of size 0x4000
keyvault decrypted OK, will use if no kv.bin is provided
decrypting SMC at address 0x1000 of size 0x3000
SMC decrypted OK, will use if no external smc.bin is provided
seeking smc config in dump...found at offset 0xf7c000! Using if no smc config is provided.
CF slot 0 decrypted ok LDV 0x13 Pairing: 0x2d9333
setting LDV from image to 19
setting pairing data from image to 0x2d9333
pairing set to: 2d 93 33
Scanning for mobile data and fsroot...Mobiles found:
    fsroot      version 02 found at offset 0x00e60000 len 0x4000 page 0x00007300
    mobileB.dat version 07 found at offset 0x00e77000 len 0x0800 page 0x000073b8
    mobileC.dat version 01 found at offset 0x00e50200 len 0x0200 page 0x00007281
    mobileE.dat version 01 found at offset 0x00e54000 len 0x0800 page 0x000072a0
extracting MobileB.dat from page 0x73b8 (offset 0xe77000), size 2048 (0x800) bytes
extracting MobileC.dat from page 0x7281 (offset 0xe50200), size 512 (0x200) bytes
extracting MobileE.dat from page 0x72a0 (offset 0xe54000), size 2048 (0x800) bytes
Statistics.settings found at offset 0xf78000, size 4096 (0x1000) bytes
seeking security files...
crl.bin found in sector 0x38d size 0xa00...verified! Will use if external file not found.
dae.bin found in sector 0x38e size 0xad30...verified! Will use if external file not found.
extended.bin found in sector 0x397 size 0x4000...verified! Will use if external file not found.
secdata.bin found in sector 0x392 size 0x400...verified! Will use if external file not found.
done!
Writing initial header to flash image

------ loading system update container ------
17502/su20076000_00000000 found, loading...done!
	Read 0xb4f000 bytes to memory
checking integrity...
header seems valid, version 2.0.17502.0
header hash is OK, checking content hashes...
content hashes seem OK, everything looks good!
extracted SUPD/xboxupd.bin (0x7ce00 bytes)
decrypting SUPD/xboxupd.bin/CF_17502.bin (0x4560 bytes)...done!
decrypting SUPD/xboxupd.bin/CG_17502.bin (0x788a0 bytes)...done!

------ Loading bootloaders and required security files ------
reading data/smc.bin failed, using smc.bin from nand dump
reset smc load address to 0x1000 size 0x3000
reading data/kv.bin failed, using kv.bin from nand dump
reading ./common/cba_9188.bin (0x1ac0 bytes)
loaded cba_9188.bin, could not check signature rsa key not present!
reading ./common/cbb_9188.bin (0x7800 bytes)
reading ./common/cd_9452.bin (0x4f20 bytes)
reading ./common/ce_1888.bin (0x5606a b pad 0x56070 b)
xell not found in perbuild directory, checking firmware /bin folder
xell not found in firmware /bin folder, checking base path
reading xell-gggggg.bin (0x40000 bytes)
extracted SUPD/xboxupd.bin/CF_17502.bin (0x4560 bytes)
extracted SUPD/xboxupd.bin/CG_17502.bin (0x788a0 bytes)
reading 17502/bin/patches_trinity.bin (0x91c bytes)
reading data/smc_config.bin failed, using smc_config.bin from nand dump
-------------------
checking smc_config
-------------------
extracting config
------------------
SMC config info:
------------------
Target temps: Cpu:  82øC Gpu:  78øC Edram:  76øC
Max temps   : Cpu:  89øC Gpu:  82øC Edram:  82øC
Cpu Fan     : 75% (overridden)
Gpu Fan     : 75% (overridden)
MAC Address : 00:22:48:c5:ef:69
AVRegion    : 0x00000100 (NTSC-M)
GameRegion  : 0x00ff (NTSC/US)
DVDRegion   : 1
resetKey    : YYLD
---------------------
Checking for smc config data patches
smc config was not patched
---------------------
could not check signature of cba_9188.bin, 1BL RSA key not present!
done!
patch slot offset reset to: 0xb0000

------ Patching BLs and modifying patches ------
Patching BLs...Done!

------ Patching boot reasons and options into flash header ------
	Patching header for xell power reason

------ Encrypting and finalizing bootloaders ------
encoding smc.bin size 0x3000
SMC checksum: 87e726b7
unknown SMC found, type: Trinity v5.1(3.01)
glitch hack found in SMC binary!
encoding kv.bin size 0x4000
decrypted keyvault has been set for reference
Master RSA pub not available, not checking hash
encoding cba_9188.bin size 0x1ac0
encoding cbb_9188.bin size 0x7800
CB 9188 seq 0x03010001 type: 0x03 cseq: 0x01 allow: 0x0001
	expected fuses:
	fuseset 00: C0FFFFFFFFFFFFFF
	fuseset 01: 0F0F0F0F0F0FF0F0 (retail slim)
	fuseset 02: F000000000000000 (sequence)
	fuseset 02: F000000000000000 (allow cseq 1)
	**dual CB flag detected!**
encoding cd_9452.bin size 0x5290
encoding ce_1888.bin size 0x56070
encoding xell-gggggg.bin size 0x40000
encoding cf_17502.bin size 0x4560
encoding cg_17502.bin size 0x788a0
encoding patches_trinity.bin size 0x550
done!

------ Adding bootloaders to flash image ------
adding smc.bin at raw offset 0x00001000 len 0x3000 (end 0x4000)
adding kv.bin at raw offset 0x00004000 len 0x4000 (end 0x8000)
adding cba_9188.bin at raw offset 0x00008000 len 0x1ac0 (end 0x9ac0)
adding cbb_9188.bin at raw offset 0x00009ac0 len 0x7800 (end 0x112c0)
adding cd_9452.bin at raw offset 0x000112c0 len 0x5290 (end 0x16550)
adding ce_1888.bin at raw offset 0x00016550 len 0x56070 (end 0x6c5c0)
adding xell-gggggg.bin at raw offset 0x00070000 len 0x40000 (end 0xb0000)
adding cf_17502.bin at raw offset 0x000b0000 len 0x4560 (end 0xb4560)
adding cg_17502.bin at raw offset 0x000b4560 len 0x788a0 (end 0xc0000, rest in fs)
adding patches_trinity.bin at raw offset 0x000c0010 len 0x550 (end 0xc0560)
Fixing up FS table...done!
Writing zeropair CG patch slot overflow data to sysupdate.xexp1
	at raw offset 0xd0000 len 0x0006ce00 (end: 0x0013ce00)...done!

------ adding 28 firmware files ------
extracted SUPD/aac.xexp (0x14000 bytes) (crc32: 0xfa1723e0 ini: 0xfa1723e0)
	adding as aac.xexp1 at raw offset 0x13ce00 len 0x00014000 (end 0x00150e00)
extracted SUPD/bootanim.xex (0x61000 bytes) (crc32: 0xe36c0e40 ini: 0xe36c0e40)
	adding as bootanim.xex at raw offset 0x154000 len 0x00061000 (end 0x001b5000)
extracted SUPD/createprofile.xex (0xc000 bytes) (crc32: 0xf24539bc ini: 0xf24539bc)
	adding as createprofile.xex at raw offset 0x1b5000 len 0x0000c000 (end 0x001c1000)
extracted SUPD/dash.xex (0x5af000 bytes) (crc32: 0x016f607b ini: 0x016f607b)
	adding as dash.xex at raw offset 0x1c4000 len 0x005af000 (end 0x00773000)
extracted SUPD/deviceselector.xex (0xa000 bytes) (crc32: 0x183f4179 ini: 0x183f4179)
	adding as deviceselector.xex at raw offset 0x773000 len 0x0000a000 (end 0x0077d000)
extracted SUPD/gamerprofile.xex (0x1b000 bytes) (crc32: 0x3feefc28 ini: 0x3feefc28)
	adding as gamerprofile.xex at raw offset 0x77e000 len 0x0001b000 (end 0x00799000)
extracted SUPD/hud.xex (0x1d000 bytes) (crc32: 0x753a9018 ini: 0x753a9018)
	adding as hud.xex at raw offset 0x79b000 len 0x0001d000 (end 0x007b8000)
extracted SUPD/huduiskin.xex (0x14000 bytes) (crc32: 0xd52ba633 ini: 0xd52ba633)
	adding as huduiskin.xex at raw offset 0x7b9000 len 0x00014000 (end 0x007cd000)
extracted SUPD/mfgbootlauncher.xex (0x8000 bytes) (crc32: 0xc8d1c074 ini: 0xc8d1c074)
	adding as mfgbootlauncher.xex at raw offset 0x7d0000 len 0x00008000 (end 0x007d8000)
extracted SUPD/minimediaplayer.xex (0xc000 bytes) (crc32: 0x4a53b32a ini: 0x4a53b32a)
	adding as minimediaplayer.xex at raw offset 0x7d8000 len 0x0000c000 (end 0x007e4000)
extracted SUPD/nomni.xexp (0xf000 bytes) (crc32: 0x97e79156 ini: 0x97e79156)
	adding as nomni.xexp1 at raw offset 0x7e4000 len 0x0000f000 (end 0x007f3000)
extracted SUPD/nomnifwk.xexp (0x2000 bytes) (crc32: 0xfd20ebe8 ini: 0xfd20ebe8)
	adding as nomnifwk.xexp1 at raw offset 0x7f3000 len 0x00002000 (end 0x007f5000)
extracted SUPD/nomnifwm.xexp (0x5000 bytes) (crc32: 0x01314c49 ini: 0x01314c49)
	adding as nomnifwm.xexp1 at raw offset 0x7f6000 len 0x00005000 (end 0x007fb000)
extracted SUPD/SegoeXbox-Light.xtt (0x6000 bytes) (crc32: 0xe0ee6049 ini: 0xe0ee6049)
	adding as SegoeXbox-Light.xtt at raw offset 0x7fd000 len 0x00006000 (end 0x00803000)
extracted SUPD/signin.xex (0x1a000 bytes) (crc32: 0x980c003b ini: 0x980c003b)
	adding as signin.xex at raw offset 0x806000 len 0x0001a000 (end 0x00820000)
extracted SUPD/updater.xex (0x7000 bytes) (crc32: 0x5f4cfb19 ini: 0x5f4cfb19)
	adding as updater.xex at raw offset 0x822000 len 0x00007000 (end 0x00829000)
extracted SUPD/vk.xex (0xb000 bytes) (crc32: 0xc2ee56b2 ini: 0xc2ee56b2)
	adding as vk.xex at raw offset 0x82b000 len 0x0000b000 (end 0x00836000)
extracted SUPD/xam.xex (0x251000 bytes) (crc32: 0x68901e82 ini: 0x68901e82)
	adding as xam.xex at raw offset 0x837000 len 0x00251000 (end 0x00a88000)
extracted nanddump/xenonclatin.xtt (0x11b000 bytes) (crc32: 0xd5d17ff5 ini: 0xd5d17ff5)
	adding as xenonclatin.xtt at raw offset 0xa89000 len 0x0011b000 (end 0x00ba4000)
extracted SUPD/xenonclatin.xttp (0x18000 bytes) (crc32: 0x7a507ad1 ini: 0x7a507ad1)
	adding as xenonclatin.xttp1 at raw offset 0xba7000 len 0x00018000 (end 0x00bbf000)
extracted nanddump/xenonjklatin.xtt (0x1a8000 bytes) (crc32: 0xdde4a14c ini: 0xdde4a14c)
	adding as xenonjklatin.xtt at raw offset 0xbc0000 len 0x001a8000 (end 0x00d68000)
extracted SUPD/xenonjklatin.xttp (0x7000 bytes) (crc32: 0xe2adddfb ini: 0xe2adddfb)
	adding as xenonjklatin.xttp1 at raw offset 0xd68000 len 0x00007000 (end 0x00d6f000)
extracted SUPD/ximecore.xex (0x17000 bytes) (crc32: 0xe232d096 ini: 0xe232d096)
	adding as ximecore.xex at raw offset 0xd6f000 len 0x00017000 (end 0x00d86000)
extracted nanddump/ximedic.xex (0x90000 bytes) (crc32: 0x1d992bfb ini: 0x1d992bfb)
	adding as ximedic.xex at raw offset 0xd87000 len 0x00090000 (end 0x00e17000)
extracted SUPD/ximedic.xexp (0x2800 bytes) (crc32: 0xfd78a3a8 ini: 0xfd78a3a8)
	adding as ximedic.xexp1 at raw offset 0xe18000 len 0x00002800 (end 0x00e1a800)
reading 17502/..\launch.xex (0xb800 bytes)
	adding as launch.xex at raw offset 0xe1a800 len 0x0000b800 (end 0x00e26000)
reading 17502/..\lhelper.xex (0x4800 bytes)
	adding as lhelper.xex at raw offset 0xe27800 len 0x00004800 (end 0x00e2c000)
reading 17502/..\launch.ini (0x3168 bytes)
	adding as launch.ini at raw offset 0xe2c800 len 0x00003168 (end 0x00e2f968)

------ adding 5 security files ------
<- Processing crl.bin ->
reading data/crl.bin (0xa00 bytes)
crl appears crypted, attempting to decrypt with CPU key...failed! Trying alternate key...success!
	adding as crl.bin at raw offset 0xe34000 len 0x00000a00 (end 0x00e34a00)

<- Processing dae.bin ->
reading data/dae.bin (0xad30 bytes)
dae appears encrypted, attempting to decrypt with CPU key...failed! Attempting to decrypt with alternate key...
success!
	adding as dae.bin at raw offset 0xe38000 len 0x0000ad30 (end 0x00e42d30)

<- Processing extended.bin ->
reading data/extended.bin (0x4000 bytes)
	adding as extended.bin at raw offset 0xe44000 len 0x00004000 (end 0x00e48000)

<- Processing fcrt.bin ->
	fcrt.bin not found and not required by keyvault, skipped

<- Processing secdata.bin ->
reading data/secdata.bin (0x400 bytes)
	adding as secdata.bin at raw offset 0xe48000 len 0x00000400 (end 0x00e48400)

------ checking for Mobile*.dat ------
MobileB.dat found, adding from previous parse
	adding MobileB.dat as type 0x31 at raw offset 0xe4c000 len 0x800 (end 0xe4c800)
MobileC.dat found, adding from previous parse
	adding MobileC.dat as type 0x32 at raw offset 0xe50000 len 0x200 (end 0xe50200)
MobileE.dat found, adding from previous parse
	adding MobileE.dat as type 0x34 at raw offset 0xe54000 len 0x800 (end 0xe54800)
Statistics.settings found, adding from previous parse
	adding Statistics.settings at raw offset 0xf78000 len 0x1000 (end 0xf79000)

------ adding smc_config.bin ------
adding smc config to offset 0x00f7c000, len 0x400

------ cleaning up image ------
Fixing up empty FS block entries...done!
Writing FS table to image offset 0xe58000 len 0x4000 (end 0xe5c000)...done!

------ finalizing image ------
fixing up big block controller on small block NAND LBA numbers...done!
calculating ECD bytes and assembling raw image...done!
done remapping!

------ writing image to disk ------
writing file 'output.bin' to disk...done!
---------------------------------------------------------------
output.bin image built, info:
---------------------------------------------------------------
Kernel    : 2.0.17502.0
Console   : Trinity
NAND size : 16MiB
Build     : Glitch
Xell      : power on console with console eject button
Serial    : 161979201705
ConsoleId : 011655167136
MoboSerial: 725665A107400175
Mfg Date  : 04/23/2010
CPU Key   : 21E0A69EB5B37CD533D13B1158C285FA
1BL Key   : DD88AD0C9ED669E7B56794FB68563EFA
DVD Key   : F33C609D604EBC71CF44E3C3C1BB8CC7
CF LDV    : 19
KV type   : type2 (hashed - unchecked, master key not available)
---------------------------------------------------------------
    xeBuild Finished. Have a nice day.
---------------------------------------------------------------
